upsd,model=CP900EPFCLCD,serial=0,status_OL=true,ups_name=fake battery_charge_low=10i,battery_charge_percent=100i,battery_charge_warning=20i,battery_mfr_date="CPS",battery_runtime_low=300i,battery_type="PbAcid",battery_voltage=24,device_mfr="CPS",device_type="ups",driver_debug=0i,driver_flag_allow_killpower=0i,driver_name="usbhid-ups",driver_parameter_pollfreq=30i,driver_parameter_pollinterval=2i,driver_parameter_port="auto",driver_parameter_product="CP900EPFCLCD",driver_parameter_productid=501i,driver_parameter_serial=0i,driver_parameter_synchronous="auto",driver_parameter_vendor="CPS",driver_parameter_vendorid=764i,driver_state="quiet",driver_version="2.8.1",driver_version_data="CyberPower HID 0.8",driver_version_internal=0.52,driver_version_usb="libusb-1.0.26 (API: 0x1000109)",firmware="",input_transfer_high=260i,input_transfer_low=170i,input_voltage=228,load_percent=13i,nominal_battery_voltage=24i,nominal_input_voltage=230i,nominal_power=540i,output_voltage=228,status_flags=8u,time_left_ns=4020000000000i,ups_beeper_status=true,ups_delay_shutdown=20i,ups_delay_start=30i,ups_mfr="CPS",ups_model="CP900EPFCLCD",ups_productid=501i,ups_serial=0i,ups_status="OL",ups_test_result="No test initiated",ups_timer_shutdown=-60i,ups_timer_start=-60i,ups_vendorid=764i
