# Fritzbox Input Plugin

This plugin gathers status information from [AVM][avm] devices (routers,
repeaters, etc) using the device's [TR-064][tr064] interface.

⭐ Telegraf v1.35.0
🏷️ network, iot
💻 all

[avm]: https://en.avm.de/
[tr064]: https://avm.de/service/schnittstellen/

## Global configuration options <!-- @/docs/includes/plugin_config.md -->

In addition to the plugin-specific configuration settings, plugins support
additional global and plugin configuration settings. These settings are used to
modify metrics, tags, and field or create aliases and configure ordering, etc.
See the [CONFIGURATION.md][CONFIGURATION.md] for more details.

[CONFIGURATION.md]: ../../../docs/CONFIGURATION.md#plugins

## Configuration

```toml @sample.conf
# Gather fritzbox status
[[inputs.fritzbox]]
  ## URLs of the devices to query including login credentials
  urls = [ "http://user:password@fritz.box:49000/" ]

  ## The information to collect (see README for further details).
  # collect = [
  #   "device",
  #   "wan",
  #   "ppp",
  #   "dsl",
  #   "wlan",
  # ]

  ## The http timeout to use.
  # timeout = "10s"

  ## Optional TLS Config
  # tls_ca = "/etc/telegraf/ca.pem"
  # tls_cert = "/etc/telegraf/cert.pem"
  # tls_key = "/etc/telegraf/key.pem"
  # tls_key_pwd = "secret"
  ## Use TLS but skip chain & host verification
  # insecure_skip_verify = false
```

### Collect options

The following collect options are available:

`device` : Collect device information like model name, SW version, uptime etc
for the configured devices. Will create `fritzbox_device` metrics.

`wan` : Collect generic WAN connection status like bit rates, transferred
bytes for the configured devices. Will create `fritzbox_wan`metrics.

`ppp` : Collect PPP connection parameters like bit rates, uptime for the
configured devices. Will create `fritzbox_ppp` metrics.

`dsl` : Collect DSL line status and statistics for the configured devices.
Will create `fritzbox_dsl` metrics.

`wlan` : Collect status and number of associated devices for all WLANs.
Will create `fritzbox_wlan` metrics.

`hosts` : Collect detailed information of the mesh network including
connected nodes, there role in the network as well as their connection
bandwidth. Will create `fritzbox_hosts` metrics.

> [!NOTE] Collecting `hosts` metrics is time consuming and generates
> very detailed data. If you activate this option, consider increasing
> the plugin's query interval to avoid interval overruns and to minimize
> the amount of collected data.

## Metrics

By default field names are directly derived from the corresponding [interface
specification][tr064].

- `fritzbox_device`
  - tags
    - `source` - The name of the device (this metric has been queried from)
    - `service` - The service id used to query this metric
  - fields
    - `uptime` (uint) - Device's uptime in seconds.
    - `model_name` (string) - Device's model name.
    - `serial_number` (string) - Device's serial number.
    - `hardware_version` (string) - Device's hardware version.
    - `software_version` (string) - Device's software version.
- `fritzbox_wan`
  - tags
    - `source` - The name of the device (this metric has been queried from)
    - `service` - The service id used to query this metric
  - fields
    - `layer1_upstream_max_bit_rate`   (uint) - WAN interface's maximum upstream
                                                bit rate (bits/sec)
    - `layer1_downstream_max_bit_rate` (uint) - WAN interface's maximum
                                                downstream bit rate (bits/sec)
    - `upstream_current_max_speed`     (uint) - WAN interface's current maximum
                                                upstream transfer rate (bytes/sec)
    - `downstream_current_max_speed`   (uint) - WAN interface's current maximum
                                                downstream data rate (bytes/sec)
    - `total_bytes_sent`               (uint) - Total number of bytes sent via
                                                the WAN interface (bytes)
    - `total_bytes_received`           (uint) - Total number of bytes received
                                                via the WAN interface (bytes)
- `fritzbox_ppp`
  - tags
    - `source`  - The name of the device (this metric has been queried from)
    - `service` - The service id used to query this metric
  - fields
    - `uptime`                  (uint) - Uptime of the PPP connection in seconds
    - `upstream_max_bit_rate`   (uint) - Maximum upstream bit rate negotiated
                                         for the PPP connection (bits/sec)
    - `downstream_max_bit_rate` (uint) - Maximum downstream bit rate negotiated
                                         for the PPP connection (bits/sec)
- `fritzbox_dsl`
  - tags
    - `source`  - The name of the device (this metric has been queried from)
    - `service` - The service id used to query this metric
    - `status`  - The status of the DLS line (Up or Down)
  - fields
    - `upstream_curr_rate`      (uint) - Current DSL upstream rate (kbits/sec)
    - `downstream_curr_rate`    (uint) - Current DSL downstream rate (kbits/sec)
    - `upstream_max_rate`       (uint) - Maximum DSL upstream rate (kbits/sec)
    - `downstream_max_rate`     (uint) - Maximum DSL downstream rate (kbits/sec)
    - `upstream_noise_margin`   (uint) - Upstream noise margin (db)
    - `downstream_noise_margin` (uint) - Downstream noise margin (db)
    - `upstream_attenuation`    (uint) - Upstream attenuation (db)
    - `downstream_attenuation`  (uint) - Downstream attenuation (db)
    - `upstream_power`          (uint) - Upstream power
    - `downstream_power`        (uint) - Downstream power
    - `receive_blocks`          (uint) - Received blocks
    - `transmit_blocks`         (uint) - Transmitted blocks
    - `cell_delin`              (uint) - Cell delineation count
    - `link_retrain`            (uint) - Link retrains
    - `init_errors`             (uint) - Initialization errors
    - `init_timeouts`           (uint) - Initialization timeouts
    - `loss_of_framing`         (uint) - Loss of frame errors
    - `errored_secs`            (uint) - Continuous seconds with errors
    - `severly_errored_secs`    (uint) - Continuous seconds with severe errors
    - `fec_errors`              (uint) - Local Modem Forward Error Correction errors
    - `atuc_fec_errors`         (uint) - Remote DSLAM Forward Error Correction errors
    - `hec_errors`              (uint) - Local Modem Header Error Control errors
    - `atuc_hec_errors`         (uint) - Remote DSLAM Header Error Control errors
    - `crc_errors`              (uint) - Local Modem Cyclic Redundancy Check error
    - `atuc_crc_errors`         (uint) - Remote DSLAM Cyclic Redundancy Check errors
- `fritzbox_wlan`
  - tags
    - `source`  - The name of the device (this metric has been queried from)
    - `service` - The service id used to query this metric
    - `wlan`    - The WLAN SSID (name)
    - `channel` - The channel used by this WLAN
    - `band`    - The band (in MHz) used by this WLAN
    - `status`  - The status of the WLAN line (Up or Down)
  - fields
    - `total_associations` (uint) - The number of devices connected to this WLAN.
- `fritzbox_hosts`
  - tags
    - `source`       - Device name this metric has been queried from
    - `service`      - Service ID used to query this metric
    - `node`         - Node name connected to the mesh network
    - `node_role`    - Node role in the network
                       ("master" = mesh master, "slave" = mesh slave, "client")
    - `node_ap`      - Name of the access point this node is connected to
    - `node_ap_role` - Access point's role  in the network
                       ("master" = mesh master, "slave" = mesh slave)
    - `link_type`    - Link type ("WLAN" or "LAN") of the peer connection
    - `link_name`    - Link name of the connection
  - fields
    - `max_data_rate_tx` (uint) - The connection's maximum transmit rate (kbits/sec)
    - `max_data_rate_rx` (uint) - The connection's maximum receive rate (kbits/sec)
    - `cur_data_rate_tx` (uint) - The connection's maximum transmit rate (kbits/sec)
    - `cur_data_rate_rx` (uint) - The connection's current receive rate (kbits/sec)

## Example Output

```text
fritzbox_device,service=DeviceInfo1,source=fritz.box uptime=2058438i,model_name="Mock 1234",serial_number="123456789",hardware_version="Mock 1234",software_version="1.02.03" 1737003520174438000

fritzbox_wan,service=WANCommonInterfaceConfig1,source=fritz.box layer1_upstream_max_bit_rate=48816000i,layer1_downstream_max_bit_rate=253247000i,upstream_current_max_speed=511831i,downstream_current_max_speed=1304268i,total_bytes_sent=129497283207i,total_bytes_received=554484531337i 1737003587690504000

fritzbox_ppp,service=WANPPPConnection1,source=fritz.box uptime=369434i,upstream_max_bit_rate=44213433i,downstream_max_bit_rate=68038668i 1737003622308149000

fritzbox_dsl,service=WANDSLInterfaceConfig1,source=fritz.box,status=Up downstream_curr_rate=249065i,downstream_max_rate=249065i,downstream_power=513i,init_timeouts=0i,atuc_crc_errors=13i,errored_secs=25i,atuc_hec_errors=0i,upstream_noise_margin=80i,downstream_noise_margin=60i,downstream_attenuation=140i,receive_blocks=490282831i,transmit_blocks=254577751i,init_errors=0i,crc_errors=53i,fec_errors=0i,hec_errors=0i,upstream_max_rate=48873i,upstream_attenuation=80i,upstream_power=498i,cell_delin=0i,link_retrain=2i,loss_of_framing=0i,upstream_curr_rate=46719i,severly_errored_secs=0i,atuc_fec_errors=0i 1737003645769642000

fritzbox_wlan,band=2400,channel=13,service=WLANConfiguration1,source=fritz.box,ssid=MOCK1234,status=Up total_associations=11i 1737003673561198000

fritzbox_hosts,node=device#17,node_ap=device#1,node_ap_role=master,node_role=slave,link_name=AP:2G:0,link_type=WLAN,service=Hosts1,source=fritz.box cur_data_rate_tx=216000i,cur_data_rate_rx=216000i,max_data_rate_tx=216000i,max_data_rate_rx=216000i 1737003707257394000
fritzbox_hosts,node=device#24,node_ap=device#17,node_ap_role=slave,node_role=client,link_name=LAN:1,link_type=LAN,service=Hosts1,source=fritz.box max_data_rate_tx=1000000i,max_data_rate_rx=1000000i,cur_data_rate_tx=0i,cur_data_rate_rx=0i 1737003707257248000
```
